** UTF-8 **
This is test release for debugging FDC (MB8877).
This contains "Japanese Communication board"(日本語通信カード) emulation.
This also contains UART emulation.
Please check if you have ROM image.
Note:
 Some names of firmwares has changed.
 See fm7.txt and fm77av.txt .
Jan 30, 2018 K.Ohta <whatisthis.sowhat@gmail.com>

Updates:
commit 6d81b4861a547c2a1f908022142953284ea26e05
Author: K.Ohta <whatisthis.sowhat@gmail.com>
Date:   Tue Jan 30 14:49:58 2018 +0900

    [VM][MB8877] Force down DRQ when LOST-DATA happens.

commit 1e1dc96ade9f4d8e6a36541049a52b414a479767
Author: K.Ohta <whatisthis.sowhat@gmail.com>
Date:   Tue Jan 30 01:44:06 2018 +0900

    [UI][Qt][MENU] DISK: Fix not affect of some entries:"Correct disk timing","Ignore CRC error" and "Immediate transfer".

commit 7b059fd0b6bd505685b030005e796e4dfa451db5
Author: K.Ohta <whatisthis.sowhat@gmail.com>
Date:   Tue Jan 30 01:00:17 2018 +0900

    [CONFIG][DISK] Fix default value ignore_crc_error and correct_disk_timing (mostly "to false").

commit ef9537b84cb7af9c472683e0d0993cb8649abf4d
Author: K.Ohta <whatisthis.sowhat@gmail.com>
Date:   Mon Jan 29 14:45:36 2018 +0900

    [DOC] Update README.en.md .

commit 829b2a9507615ba4eabdd927f42c2cc73ea0085a
Author: K.Ohta <whatisthis.sowhat@gmail.com>
Date:   Mon Jan 29 14:44:16 2018 +0900

    [DOC] Update (GITHUB's) README.md.

commit 583d6c628d90055925fa5a7b697a52e60e0052ee
Author: K.Ohta <whatisthis.sowhat@gmail.com>
Date:   Mon Jan 29 10:41:33 2018 +0900

    [VM][FM77AV40] Fix FTBFS with Fedora linux.

commit a9157933c5b4761f29290ba7f8aae06f49880156
Author: K.Ohta <whatisthis.sowhat@gmail.com>
Date:   Mon Jan 29 10:35:03 2018 +0900

    [VM][MB8877] TRY: Add (temporally) debug log to check DRQ timing for FLEX.
    [VM][MB8877][FM77AV] No need to hack with PSY-O-BLADE.This is test delete.

commit 0a5a54e56ddcca52a239c68d2c3786b388319fe0
Author: K.Ohta <whatisthis.sowhat@gmail.com>
Date:   Mon Jan 29 10:34:25 2018 +0900

    [VM][FM7][DISK] Fix RPM value of 2D/2DD drive to 300rpm.

